CRJ 700 Checklist

Created: 12/29/2011

# Tasks:

☐ **Start Up**

☐ **Clearence**

☐ **File Flight**

☐ **Flight Plan**

☐ **FMS**

☐ **APU Gen On**

☐ **APU Start/On**

☐ **Battery On**

☐ **Avonics On**

☐ **Engine Start**

☐ **Fuel Flow**

☐ **APU Gen Off**

☐ **Lights On**

☐ **Fuel Pump On**

☐ **Fuel Pumps Off**

☐ **Generator On**

☐ **Inverter On**

☐ **Pushback**

☐ **Transponder On**

☐ **Pre-Flight**

☐ **12-20kts**

☐ **Acars**

☐ **Taxi**

☐ **Taxi Clearence**

☐ **Autopilot**

☐ **Takeoff**

☐ **Takeoff Clearence**

☐ **Autopilot On**

☐ **Brake**

☐ **Flaps 8 degrees**

☐ **Throttle**

☐ **Airborne**

☐ **Acars**

☐ **Apu Off**

☐ **Avonics Off**

☐ **Battery Off**

☐ **Engines Off**

☐ **Generators Off**

☐ **Inverter Off**

☐ **Lights Off**

☐ **12-20kts**

☐ **Autopilot Off**

☐ **Flaps**

☐ **Off Runway**

☐ **Reverse -> 60kts**

☐ **Spd Brake**

☐ **Taxi Clearence**

☐ **146kts**

☐ **Flaps**

☐ **Gear**

☐ **ILS/APP**

☐ **Spd Brake**

☐ **250kts**

☐ **5 degree descent**

☐ **Via Arrival**

☐ **Flight Plan Level**

☐ **Mach 0.81**

☐ **250kts**

☐ **Autopilot Engage**

☐ **Flaps**

☐ **Gear**

☐ **Via Departure**